1.

The DAA means Decimal Adjust after Addition. DAA instruction allows addition of numbers represented in 8-bit packed BCD code. It is used immediately after normal addition instruction operating on BCD codes.

2.